**Nimonic 105 Grain Structure**









For an 8000C Hot Tensile Test:

UTS or YS= 100 KSI and % Elongation= 41